File systems <https://en.wikipedia.org/wiki/File_system>

A file system manages data accessed on a storage device.   
Each operating system (OS) has its own system for handling files. *Some* OSs are able to read *some* other OSs file systems with limitations but that should not be assumed.  
An analogy: a driver who knows the rules of the road (operating system) and can operate a vehicle (storage device with a file system).

In most parts of the world and in most cars, a driver gets into a car through the front door on the left side expecting to see a steering wheel and controls in the same locations as in almost every other car.

Imagine a Canadian getting into a car England. 'What the heck is the steering wheel doing *over there*?' or '*over here?*' if you are a passenger. To use a car well, the car's controls must be suited to the country where the car is driven. In computer terms, what is the file system of the car? It is either for left-hand or right-hand drive.

Now that you are driving a car, you come to a roundabout: do you go clockwise or counterclockwise? It depends on which side of the road they drive in that country. Who has the right-of-way: the traffic already circling the roundabout or traffic coming into it? (it should be the former – the latter caused lots of problems.)



The driver must know the rules of the road in order to operate the car safely. An empty road looks much the same in Canada as in England; there are few, if any, clues on the road itself as to which side to drive on. Knowing how to use the road is important so as not to crash into others.

|  |  |
| --- | --- |
| Car driving on highway surrounded by picturesque mountains. |  |

Tourists in London, England are injured all the time as they cross the road; they look left, see no cars coming, and step off the curb into the road where the cars come from the right.

You have to know how to use the physical hardware (the car) *and* the logical operation of it (rules of the road). If you plug a metaphorical car into a United Kingdom road OS, the OS will recognize cars only with right-hand drive; plug into a Canadian road OS and only left-hand drive cars are recognized. Trains and boats, although vehicles, are never recognized for driving on roads because…well, just because.

**The operating system has to know how to recognize and use the physical hardware (the storage device via low level software called a "driver" coincidently) and the logical operation of it to find and open a file and then read and write data to the file.**

The process of the OS recognizing a storage device so it can use it is called ***mounting***. (The spare wheel & tire in the car's trunk/boot does not become useful until it is mounted in place of the wheel with the flat tire. Snow tires are not useful until they are mounted on wheels and the wheels mounted on your car.) When the OS mounts a drive, it recognizes the logical file system on the attached physical storage device. The way the file system is presented to the end user through the file browser looks very much the same on most systems – a hierarchical organization beginning at the drive letter or root with multiple levels of directories or folders containing sets of files.

<https://en.wikipedia.org/wiki/Mount_(computing)>

An example of a hierarchical system from Botany:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Kingdom | Phylum | Class | Order | Family | Genus | Species |
| *Animalia* | *Chordata* | *Mammalia* | *Primata* | *Hominidae* | *Homo* | *Sapiens* |

The concept of hierarchical filesystems are derived from paper filing systems:

* Office building – XYZ Company
  + Departments – Sales, Warehouse, Accounting
    - Filing cabinets – Orders, Invoices
      * Drawers – labeled A-L, M-Z indicating an alphabetic index, the method of accessing the cabinet's contents
        + Folders – by Customer name

File(s) – by order number  
(cross reference of order numbers to customer name maintained in Orders filing cabinet)

Each company has a file system but each company may organize it differently. Without knowing the company's method of organization, how would you find anything quickly?

Computer file systems organize your files. IBM, Microsoft, Apple, and Linux all use their own proprietary systems which have, of course, limited compatibility with each other. Each file system has different structure and logic, has different properties for files (e.g. filename length, pathname length, allowable characters for names and case sensitivity, max file size), security attributes, and more.

Optical discs usually use ISO 9660 file system because optical discs were designed for "cross-platform compatibility". USB flash drives are formatted (as FAT32 by default) for cross-platform compatibility.

Operating systems enable file access, directory/folder operations, and authorization security via the **logical file system** which connects software applications with the data within files. The logical file system provides a uniform application program interface (API) for file operations — OPEN, CLOSE, READ, etc., and passes the requested operation to the physical layer it for processing on the storage device.

The **physical file system** layer is concerned with the mechanical/electrical operation of the storage device. It processes physical blocks being read or written. It handles buffering and memory management and is responsible for the physical placement of blocks in specific locations on the storage medium. The physical file system interacts with the device drivers to control the storage device according to Operating System requests.

Location of storage devices:

* [DAS](https://en.wikipedia.org/wiki/Direct-attached_storage): Direct Attach Storage – local devices (internal HDD & SSD, external plug-ins like USB and optical) attached through an internal bus adapter/driver. DAS has a one-to-one relationship between each storage device and the host (PC or server). For non-removable internal devices, the OS must provide formatting and a file system to enable file-level access. Most removeable external devices are preformatted with a cross-platform compatible filesystem.
* [NAS](https://en.wikipedia.org/wiki/Network-attached_storage): Network Attached Storage is file-level computer data storage through a network protocol which effectively appears to the OS as a native file system but the actual implementation is hidden inside the NAS appliance. A single NAS will support different file access protocols for multiple OSs over a standard TCP/IP network.
  + e.g. a home office NAS will store a file accessible to both Windows and macOS systems, most will provide file access over the Internet.
  + Used for data sharing among many users on heterogeneous systems on the same intranet in Small to Medium sized Enterprises (SMEs).
* [SAN](https://en.wikipedia.org/wiki/Storage_area_network) - SANs separate computing from storage. Storage Area Network is block-level computer data storage through a special protocol on a dedicated connection/network which effectively appears to the OS as a raw storage device. The OS must provide formatting and a file system to enable file-level access. SAN is more similar to DAS than NAS. The difference between SAN and DAS is the attachment of the storage device, SAN through a connection (iSCSI) to external storage, DAS through a local connection (SCSI) to internal storage.
  + high performance, flexibility, and complexity for large enterprises and cloud services
* NAS and SAN can provide automatic backup and snapshotting, storage reliability and redundancy, and scalability. DAS requires the host server and administrator to provide those functions.
* cloud providers can provide both NAS and SAN services remotely.
* <https://serverfault.com/questions/81723/what-is-the-difference-between-san-nas-and-das>

Critical features of contemporary OS file systems *except FAT32, exFAT*

* File Metadata: Windows Properties / Linux stat / macOS xattr
* Security, Data Integrity (controlling multiple applications attempting to access the same file), Crash protection (journaling), Encryption, Compression
* Snapshot capability for regressing system to previous state. For efficiency, snapshots record only the incremental changes made since the previous snapshot. [Flat](https://searchdatabackup.techtarget.com/definition/flat-backup) [Backup](https://searchdatabackup.techtarget.com/feature/The-flat-backup-or-backup-less-backup-data-protection-option) systems take advantage of this.

|  |  |  |  |
| --- | --- | --- | --- |
| Filesystem | **MS Windows** | **Apple macOS** | **Linux** |
| [**NTFS**](https://en.wikipedia.org/wiki/NTFS) | Native | native read-only,  3rd party utility for writing and management | |
| [**APFS**](https://en.wikipedia.org/wiki/Apple_File_System) | 3rd party utility | Native | 3rd party utility |
| [**ZFS**](https://en.wikipedia.org/wiki/ZFS)**,** [**ext4**](https://en.wikipedia.org/wiki/Ext4) | Paragon ExtFS (3rd party utility) | | Native |
| [**FAT32**](https://en.wikipedia.org/wiki/File_Allocation_Table#FAT32) | Native read/write but 4 GB file size limit, slower I/O. USB storage constraints tolerated for "cross-platform compatibility" | | |
| [**exFAT**](https://www.howtogeek.com/235596/whats-the-difference-between-fat32-exfat-and-ntfs/)[**32 vs ex**](https://www.pcworld.com/article/3109559/why-your-usb-drives-file-format-matters-fat32-vs-exfat-vs-ntfs.html) | Native, MS proprietary format | | 3rd party utility and/or licensing |
| [**Optical**](https://en.wikipedia.org/wiki/ISO_9660) | ISO 9660 designed for "cross-platform compatibility" | | |

Enterprise and high-performance computing file systems:

* [IBM Spectrum Scale](https://en.wikipedia.org/wiki/IBM_Spectrum_Scale)
* [Lustre](https://en.wikipedia.org/wiki/Lustre_(file_system)) – Linux Cluster
* [Apache Hadoop](https://en.wikipedia.org/wiki/Apache_Hadoop)

<https://en.wikipedia.org/wiki/Comparison_of_file_systems>

Storage devices

<https://www.backblaze.com/b2/hard-drive-test-data.html> <https://www.backblaze.com/blog/>

<https://www.zdnet.com/article/ssd-reliability-in-the-real-world-googles-experience/>  
evidence that consumer grade HDD and SSD are as reliable as enterprise/server grade.

|  |  |  |
| --- | --- | --- |
|  | **Reliability reduced by** | **Failure risk** |
| **HDD** Hard Disk DriveLow capital cost per GB  High operating cost due to drive motor and waste heat to be cooled | Usage | Drive loss > Data loss addressed with RAID redundancy and MAID Massive Array Of Idle Drives in large storage systems. |
| **SSD** Solid State Drive  High capital cost per GB  Low operating cost due to no moving parts and minimal heat emissions | Age - need filesystem with data checksum.  IBM Spectrum/GPFS,  Linux ZFS.  Diagnostic utilities needed on Win10, macOS, Linux which, ironically, can reduce the life of drives due to additional intensive use. | Data loss > Drive loss SSD back up *more* important than with HDD |